|  |  |
| --- | --- |
| General information Customer | SHIPMENT TO |
| Company name |  |  **Synergy Health Utrecht B.V.** De Liesbosch 88 3439 LC Nieuwegein The Netherlands |
| Contact person |  |
| Email address |  |
| Phone number |  |
| Add. Remarks CoA  |

|  |  |
| --- | --- |
| **Product information**  |  **AREA FOR LABEL** |
| Article name  |  |  |
| Product Type(tubing, catheter, drape etc.) |  |
| Batch number |  |
| Reference to order(PO number)\* |  |
| **Quote number**\*\*  |  [ ]  N/A |

*\* Please note; requests without a PO number cannot be processed.*

*\*\*Please note: without a valid quotation number standard catalogue price will be applicable.*

 *The quote number can be found on your quote.*

\*\*\* NEXT PAGE \*\*\*

|  |
| --- |
| **Sample and test information** |
| **Please note:** Attach a picture or schematic of the sample to be tested as appendix. |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1** | **Product Reference/Batch number** | **Purity** | **Extraction type** | **Extraction time**  | **Extraction temperature** |
|  | [ ] EO[ ] ECH[ ] EG | [ ] Cut up and immerse[ ] Static fluid path[ ] Other:  | [ ] Exhaustive[ ] Specific: hrs | [ ] 20 - 25°C[ ] 37°C[ ] Other: °C |
| Remarks¹ |
| Contact area cm² [ ] N/A | Number of samples to be tested |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **2** | **Product Reference/Batch number** | **Purity** | **Extraction type** | **Extraction time**  | **Extraction temperature** |
|  | [ ] EO[ ] ECH[ ] EG | [ ] Cut up and immerse[ ] Static fluid path[ ] Other: | [ ] Exhaustive[ ] Specific: hrs | [ ] 20 - 25°C[ ] 37°C[ ] Other: °C |
| Remarks¹ |
| Contact area cm² [ ] N/A | Number of samples to be tested |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **3** | **Product Reference/Batch number** | **Purity** | **Extraction type** | **Extraction time**  | **Extraction temperature** |
|  | [x] EO[ ] ECH[ ] EG | [ ] Cut up and immerse[ ] Static fluid path[ ] Other: | [ ] Exhaustive[ ] Specific: hrs | [ ] 20 - 25°C[ ] 37°C[ ] Other: °C |
| Remarks¹ |
| Contact area cm² [ ] N/A | Number of samples to be tested |
| **Additional Remarks** |

¹ Analysis will be performed on full content within packaging unless otherwise specified (excluding mounting cards, IFU’s or other paper based materials)

\*\*\* NEXT PAGE \*\*\*

|  |  |  |
| --- | --- | --- |
| Specify Acceptable Residual limits according to **ISO 10993-7** | [ ]  Limited exposure device <24h[ ]  Permanent contact device >30d [ ]  Other: | [ ]  Prolonged exposure device >24h <30d[ ]  Tolerable contact limits: μg/cm2 |
| Testing post sterilisation [ ]  1 [ ]  2 [ ]  3 Postconditioning Time hrs |

|  |  |  |
| --- | --- | --- |
| **Sample Handling** | [ ]  Normal (10 working days target) | [ ]  Priority (additional costs)Only on advance notice, confirmation by Synergy Health Utrecht required.Please mark the shipping box with **PRIORITY.** |

|  |  |  |
| --- | --- | --- |
| **Sample storage conditions** | [ ]  -20°C ± 5°C[ ]  Ambient temperature | Temperature logger enclosed [ ]  Yes [ ]  No Return address: |
| **Please note:** Samples will be disposed after analysis are reported. |

|  |  |  |  |
| --- | --- | --- | --- |
| Signature Customer: |  | Date: |  |